Reference Access and Interconnection Offer Sub Annex C-FI 10 Fixed Call Transit Services

Table of Contents

[1 General 3](#_Toc452284421)

[2 Definitions 4](#_Toc452284422)

[3 Omantel Fixed Call Cascade Transit Services 5](#_Toc452284423)

[4 Routing Regimes 6](#_Toc452284424)

[5 Ordering and Delivery 7](#_Toc452284425)

[6 Tariff 8](#_Toc452284426)

[7 Fault Management 9](#_Toc452284427)

[8 Forecasts 10](#_Toc452284428)

# General

* 1. This Sub Annex sets out the Fixed Call Transit Services.
	2. The Requesting Party shall request for Fixed Ancillary Interconnect Services to be able to convey calls between Omantel and the Requesting Party.
	3. The Parties shall agree in advance to all necessary technical requirements, including Call set-up and clear-down sequences, for the conveyance of Calls pursuant to this Sub Annex.
	4. The Parties shall convey Calls during those periods of time and at the same standard and quality of Service as Parties convey similar Calls to their customers.
	5. Omantel shall be under no obligation to convey Transit Calls to destinations that are not available to Omantel Customers and not agreed between both Parties.
	6. The Requesting Party shall not hand over to Omantel and Omantel shall be under no obligation under this Sub Annex, to convey Transit Calls not listed in the Omantel Transit Price List as being available to the Requesting Party.
	7. Each Party shall correct faults that occur in its Network which affect the conveyance of Calls in accordance with such Party’s normal engineering practices. For the avoidance of doubt, neither Party warrants that its Network is, or will be, free from faults.

# Definitions

* 1. The definitions in Annex L shall apply to this Sub Annex in addition to the following definitions:
		1. Region – refer to definitions of Regions in the Sub Annex C-FI 01, Fixed Ancillary Interconnection Services.

# Omantel Fixed Call Cascade Transit Services

* 1. Omantel offers Services to transit traffic originated from the Requesting Party Network and terminating on a Third Party Network and vice versa.
	2. The Requesting Party and Third Party operator do not have a separate agreement between them. Omantel executes mediation and billing of termination fees. Omantel invoices the Requesting Party the termination fee of the Third Party Operator plus the transiting fee and administrative fee and any additional charges set by the Third Party Operator and administration fee listed in Clause ‎7 of this Sub Annex. The Requesting Party shall also pay for additional Port Capacity and the relevant services where required. The termination fee and any other charges set by the Third Party Operator are paid in full to the Third Party Operator.
	3. In this Clause the GMP1 Tandem switch is considered to be an equivalent to an Omantel Primary Switch.

# Routing Regimes

* 1. To fixed termination points
		1. Calls handed over from the Requesting Party Network to the Omantel Network designated to be transited through Omantel Network and terminated at a Third Party Network shall be handed over at the Point of Interconnection specified by Omantel.

# Ordering and Delivery

* 1. Ordering and delivery shall be handled according to Annex H.

# Tariff

* 1. The up to date tariff for the Services can be found in Annex M.
	2. The cost of additional product features, specialized billing, systems and/or network interfaces, non-standard connectivity and associated configuration, integration and testing are not included in the published tariffs. Such cases will be dealt with on a case-by-case basis against mutual agreed timelines and charges.

# Fault Management

* 1. Fault Management shall be handled according to Annex H.

# Forecasts

* 1. Forecasting shall be handled according to Annex F.